**16 DEPARTMENT OF PUBLIC SAFETY**

**219 OFFICE OF STATE FIRE MARSHAL**

**Chapter 5: PORTABLE FIRE EXTINGUISHERS**

**SUMMARY**: This summary is taken from the incorporated materials. “The provisions of this standard apply to the selection, installation, inspection, maintenance, and testing of portable extinguishing equipment. The requirements given herein are minimum. Portable extinguishers are intended as a first line of defense to cope with fires of limited size. They are needed even though the property is equipped with automatic sprinklers, standpipe and hose, or other fixed protection equipment. They do not apply to permanently installed systems for fire extinguishment, even though portions of such systems are portable (such as hose and nozzles attached to a fixed supply of extinguishing agent).”

1. This agency incorporates by reference the National Fire Protection Association (NFPA) Standard # 10, *Standard for Portable Fire Extinguishers*, 2018 edition. All rights reserved by the National Fire Protection Association. Copies of NFPA Standard #10 are available through the National Fire Protection Association, 1 Batterymarch Park, Quincy, MA 02269.

STATUTORY AUTHORITY: 25 M.R.S.A. §2452

EFFECTIVE DATE:

 December 22, 1977 (filed September 27, 1978)

EFFECTIVE DATE (ELECTRONIC CONVERSION):

 May 15, 1996

REPEALED AND REPLACED:

 August 7, 2001

AMENDED:

 September 1, 2003 - filing 2003-293

 March 17, 2009 – filing 2009-103, NFPA Standard #10 updated to 2007 edition

 April 17, 2021 – filing 2021-074, NFPA Standard #10 updated to 2018 edition